|  |
| --- |
| ACTS |
| Advanced Low-level Controller – ALC 3.0 |
| Install Manual |
|  |
| **[键入作者姓名]** |
| **2019/9/26** |

|  |
| --- |
| ACTS Technologies Inc. |

Contents

[1 Overview 3](#_Toc21509618)

[1 Operating System 3](#_Toc21509619)

[2 Download and install NI-DAQmx driver 3](#_Toc21509620)

[3 Supply your Hardware info 4](#_Toc21509621)

[4 Copy and Install 4](#_Toc21509622)

[5 Update new version and Help documents 4](#_Toc21509623)

# 1 Overview


The purpose of this document is to familiarize the user with the operation of the ACTS Advanced Low-level Controller – ALC 3.0.

# 1 Operating System

Windows 10.

# 2 Download and install NI-DAQmx driver

NI-DAQmx provides support for customers using NI data acquisition and signal conditioning devices.



# 3 Supply your Hardware info

At command line window, enter “ipconfig /all”, and copy output info to ACTS.

At c:\>, enter “dir /w”, and copy output info to ACTS.

# 4 Copy and Install

Copy all software to c:\acts.

# 5 Update new version and Help documents

<https://github.com/MingJing2015/ACTS-update>

If you have any questions regarding this manual, please contact ACTS.